,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SupEqui##OTHER##,Light Source##OTHER##
Solegra D4 OTA 24000-840 ETDD + ZS A 5075/3000,1.2,0,0.12,10173886 + 10173922,7140351 + 7131000,RAL9016 Verkehrsweiß,19.7,http://www.trilux.com/TOC/7140351,I,IP40,ETDD,LED,168,80,45 76 93 91 99 25 52 77 9,23600,4000,TRILUX_RAL9016,TRILUX_WH_4000_opak,Solegra_D4_ZS_A : 5075/3000,Solegra_LS : TX063024
