,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO_1##OTHER##,SEO_2##OTHER##,leo_offset##LENGTH##METERS,Light Source##OTHER##
Skeo R W2 GT SE4R/2000-730 1G1P ET,0.15,0.3,0.15,10158137,6966540,DB703 Anthrazit,3.7,http://www.trilux.com/TOC/6966540,Schutzklasse I,IP65,ET,LED,19,70,1999,3000,TRILUX_Alu_DB703,TRILUX_3000_Skeo_R,TRILUX_Alu_DB703,0.075,Skeo_R_W_LS : TX054495
