,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SupEqui_Mat##OTHER##,SupEqui##OTHER##,Light Source##OTHER##
Solegra D4 OTA 24000-830 ET + D4 ZP 01,1.2,0,0.12,10173881 + 10176496,7140240 + 7172100,RAL9016 Verkehrsweiß + RAL9016 Verkehrsweiß,20.5,http://www.trilux.com/TOC/7140240,I,IP40 + IP20,ET,LED,168,80,46 78 95 95 100 45 77 94 5,19800,3000,TRILUX_RAL9016,TRILUX_WH_3000_opak,TRILUX_RAL9016,Solegra_D4_ZP : 01,Solegra_LS : TX062790
