,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Creavo M48-TS LW19-03 62-840 ETDD 01,1.497,0.297,0.043,10226172,7636251,RAL9016 Verkehrsweiß ,6.5,http://www.trilux.com/TOC/7636251,II,IP20,ETDD,LED,37,80,89 100 100 100 100,6200,4000,TRILUX_RAL9016,TRILUX_WH_4000,Creavo_LS : TX195314
