,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
CreavoAct M84-TS LW19-03 42-8 ETDD8 01 (ActDCW),0.622,0.622,0.043,10228981,7615662,RAL9016 Verkehrsweiß ,4.8,http://www.trilux.com/TOC/7615662,I,IP20,ETDD8,LED,35,80,89 100 100 100 100,4200,6500,TRILUX_RAL9016,TRILUX_WH_6500,Creavo_LS : TX195486
