,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,SupEqui##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
SFlow C2-L LW19 4000-830 ET 01,1.413,0.1,0.045,10225275,7572740,RAL9016 Verkehrsweiß,3.97,http://www.trilux.com/TOC/7572740,I,IP20,ET,LED,27,80,66 88 96 90 100 21 47 74 10,4000,3000,C-L_LW19,TRILUX_RAL9016,TRILUX_WH_3000,SFlow_C_LS : TX150309
