,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Kratex HE 1200 40-840 ET PC EB3,1.36,0.157,0.197,10169111,7668740,RAL1003 Signalgelb ,10.6,http://www.trilux.com/TOC/7668740,I,IP66,ET,LED,45,80,42 71 89 94 100 0 0 17 6,4900,4000,TRILUX_RAL1003,TRILUX_WH_4000,Kratex_LS : TX199620
