,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,SupEqui##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
SFlow H2-L CDP-I 6300-830 ETDD 03,1.413,0.1,0.07,10198456,7358551,RAL9006 Weißaluminium,4.65,http://www.trilux.com/TOC/7358551,I,IP20,ETDD,LED,52,80,80 96 99 99 100 27 64 91 1,6300,3000,H-L_CDP,TRILUX_RAL9006,TRILUX_WH_3000,SFlow_H_LS : TX133396
