,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Duroxo G2 B LED6500-840 ET,1.310,0.123,0.123,10173305,7115440,Duroxo_G2_End_cap,Transparent,4.2,http://www.trilux.com/TOC/7115440,,,ET,LED,46,80,37 75 94 98 100 4 16 28 2,6699,4000,TRILUX_Alu_RAL_7001,TRILUX_4000_Duroxo,Duroxo_LS : TX055828
