,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,RegPrim##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Mirona Fit-Spo 2L TB 130-840 ETDD,0.32,0.342,0.065,10148603,6918651,Mirona_Fit_GH : 2_LED_Module,RAL9016 Verkehrsweiß,4.26,http://www.trilux.com/TOC/6918651,I,IP65,ETDD,LED,82,80,76 95 100 100 100 0 0 0 0,13300,4000,TRILUX_RAL9016,TRILUX_WH_4000,Mirona_Fit_Spo_LS : TX263665
Mirona Fit-Spo 2L TB 130-940 ETDD,0.32,0.342,0.065,50241751,7699551,Mirona_Fit_GH : 2_LED_Module,RAL9016 Verkehrsweiß,4.26,http://www.trilux.com/TOC/7699551,I,IP65,ETDD,LED,111,90,76 95 100 100 100 0 0 0 0,13300,4000,TRILUX_RAL9016,TRILUX_WH_4000,Mirona_Fit_Spo_LS : TX200042
Mirona Fit-Spo 4L TB 260-840 ETDD,0.65,0.342,0.065,10148604,6918751,Mirona_Fit_GH : 4_LED_Module,RAL9016 Verkehrsweiß,8.06,http://www.trilux.com/TOC/6918751,I,IP65,ETDD,LED,157,80,76 95 100 100 100 0 0 0 0,26700,4000,TRILUX_RAL9016,TRILUX_WH_4000,Mirona_Fit_Spo_LS : TX263666
Mirona Fit-Spo 4L TB 260-940 ETDD,0.65,0.342,0.065,50221956,7667251,Mirona_Fit_GH : 4_LED_Module,RAL9016 Verkehrsweiß,8.06,http://www.trilux.com/TOC/7667251,I,IP65,ETDD,LED,222,90,76 95 100 100 100 0 0 0 0,26400,4000,TRILUX_RAL9016,TRILUX_WH_4000,Mirona_Fit_Spo_LS : TX200043
