,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,Light Source##OTHER##
SNS RH7-2R HRXFL-22 20-840 ETDD 01,0.206,0,0.175,10193013,,RAL9016 Verkehrsweiß,3.66,http://www.trilux.com/TOC/9002018781,I,IP20,ETDD,LED,18,80,79 99 100 100 100,2000,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_HR,SNS_LS : TX102395
SNS RH7-2R MRVFL-19 20-840 ETDD 01,0.206,0,0.175,10193588,,RAL9016 Verkehrsweiß,3.66,http://www.trilux.com/TOC/9002019225,I,IP20,ETDD,LED,17,80,95 100 100 100 100,2000,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_MR,SNS_LS : TX102397
SNS RH7-2R MRVFL-19 20-830 ETDD 01,0.206,0,0.175,10194759,,RAL9016 Verkehrsweiß,3.66,http://www.trilux.com/TOC/9002020152,I,IP20,ETDD,LED,19,80,95 100 100 100 100,2000,3000,TRILUX_RAL9016,TRILUX_WH_3000,TRILUX_MR,SNS_LS : TX102396
