,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Light Source##OTHER##,SEO##OTHER##,Mat##OTHER##,Ref##OTHER##,rotatable##OTHER##
8521 RMS1L/700-amber 1G1 ET 05,0.212,0,0.266,10130075,6491040,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6491040,Schutzklasse I,IP68,ET,LED,13,,699,amber,Lutera_LS : TX046291,TRILUX_WH_amber_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
