,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,SupEqui_SEO##OTHER##,SupEqui##OTHER##,Light Source##OTHER##
SNS RC5 HRW 20-940 ETDD 01,0.165,0,0.13,10183597,,RAL9016 Verkehrsweiß,1.11,,I,IP20,ETDD,LED,26,90,71 95 100 100 100,2100,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_HR,TRILUX_PC-T,Sonnos_RC5_W_no_accessories,Sonnos_LS : TX068802
SNS RC5 HRW 20-940 ETDD 01 + RC05 ZIP54-PC-T-T,0.165,0,0.13,10183597 + 10179650,7188600,RAL9016 Verkehrsweiß,1.179,,I,IP20 IP54,ETDD,LED,26,90,71 95 100 100 100,2100,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_HR,TRILUX_PC-T,Sonnos_RC5_ZIP54,Sonnos_LS : TX068969
