,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,SupEqui_SEO##OTHER##,SupEqui##OTHER##,Light Source##OTHER##
SNS QC1 WRMF-19 8-930 ETDD 01,0.075,0.075,0.08,10182186,,RAL9016 Verkehrsweiß,0.41,,II,IP20,ETDD,LED,10,90,99 100 100 100 100,800,3000,TRILUX_RAL9016,TRILUX_WH_3000,TRILUX_RAL9016,TRILUX_PC-T,Sonnos_QC1_no_accessories,Sonnos_LS : TX068745
