,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
OleveonF 15 B 26-74/16 ML-840 ET PC (Stage E),1.552,0.102,0.091,10229803,7663440,RAL7035 Lichtgrau,2.5,http://www.trilux.com/TOC/7663440,I,IP66,ET,LED,54,80,56 85 95 93 100 0 0 11 7,7400,4000,TRILUX_RAL7035,TRILUX_WH_4000,OleveonF_LS : TX194540
