,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,PrimEqui##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,MatSupEqui##OTHER##,SEO##OTHER##,Light Source##OTHER##
ArimoFit M48 PW19 63-830 ETDD,1.497,0.297,0.02,10216495,7531651,ArimoFit_M46_ M48_M57_M59_M73_M84,ArimoFit_no_accessories,RAL9016 Verkehrsweiß,4.2,http://www.trilux.com/TOC/7531651,II,IP40,ETDD,LED,52,80,65 89 97 100 100 0 0 0 0,6000,3000,TRILUX_RAL9016,TRILUX_RAL9016,TRILUX_WH_3000,ArimoFit_LS : TX149924
