,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Ref##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
7651IP PVN 120-840ETDD L150 01,1.474,0.063,0.091,10247399+10241408,9002116391+7789600,RAL9016 Verkehrsweiß,0,http://www.trilux.com/TOC/9002116391,I,IP50+IP50,ETDD,LED,86,80,70 89 96 93 100 15 39 67 7,12600,4000,7651_IP50_P,TRILUX_RAL9016,TRILUX_WH_4000,7651_LS : TX264480
