,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Lunexo H1 CDP-I 6500 840 ETDD +LLWC 01,1.203,0.2,0.045,10143007;,6826451;,Lunexo_H_GH,Verkehrsweiß RAL 9016;,9,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6826451,Schutzklasse I;,IP20;,ETDD,LED,61,80,6.099,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX050911
