,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Ref##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
7651IP HE LVW 60-865ETDD L150 01,1.474,0.063,0.062,10246125+10241408,9002115101+7789600,RAL9016 Verkehrsweiß,0,http://www.trilux.com/TOC/9002115101,I,IP50+IP50,ETDD,LED,34,80,53 86 97 98 100 0 0 33 2,6300,6500,7651_IP50_L,TRILUX_RAL9016,TRILUX_WH_6500,7651_LS : TX264918
