,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Solegra WD1 OTA 2600-830 ETDD + WD1 ZP C1/C,0.4,0,0.12,10173763 + 10173931,7132951 + 7131900,RAL9016 Verkehrsweiss + RAL9016 Verkehrsweiss,5.5,http://www.trilux.com/TOC/7132951,I,IP40 + IP20,ETDD,LED,19,80,46 78 95 100 100,2100,3000,TRILUX_RAL9016,TRILUX_WH_3000_opak,Solegra_LS : TX062852
