,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SEO_2##OTHER##,Light Source##OTHER##
SFlow C1-L MRW LED3200-830 ET 01,1.132,0.1,0.045,10141009,6892740,MRW_MRX : MRW,Verkehrsweiß RAL 9016,3.2,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6892740,Schutzklasse I,IP20,ET,LED,26,80,2999,3000,TRILUX_Alu_RAL_9016,TRILUX_SFlow_3000,TRILUX_SFlow_3000_outer,Solvan Flow_C_LS : TX050940
