,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SupEqui##OTHER##,Light Source##OTHER##
Solegra D4 OTA 24000-830 ETDD + ZS DB 5075/6000,1.2,0,0.12,10173884 + 10173930,7140251 + 7131800,RAL9016 Verkehrsweiß + RAL9016 Verkehrsweiß,21.14,http://www.trilux.com/TOC/7140251,I,IP40 + IP20,ETDD,LED,168,80,45 76 93 91 99 25 52 77 9,22400,3000,TRILUX_RAL9016,TRILUX_WH_3000_opak,Solegra_D4_ZS_DB : 5075/6000,Solegra_LS : TX063017
