,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO_1##OTHER##,SEO_2##OTHER##,leo_offset##LENGTH##METERS,Light Source##OTHER##
Skeo R W1 GS SE2R/700-730 1G1P ET,0.1,0.2,0.1,10158134,6966240,DB703 Anthrazit,1.3,http://www.trilux.com/TOC/6966240,Schutzklasse I,IP65,ET,LED,11,70,700,3000,TRILUX_Alu_DB703,TRILUX_3000_Skeo_R,TRILUX_Alu_DB703,0.05,Skeo_R_W_LS : TX054488
Skeo R W1 GS SE2R-SE2R/1500-730 1G1P ET,0.1,0.2,0.1,10158135,6966340,DB703 Anthrazit,1.3,http://www.trilux.com/TOC/6966340,Schutzklasse I,IP65,ET,LED,23,70,1499,3000,TRILUX_Alu_DB703,TRILUX_3000_Skeo_R,TRILUX_3000_Skeo_R,0.0,Skeo_R_W_LS : TX054489
Skeo R W1 GT AB18R/1600-730 1G1P ET,0.1,0.2,0.1,10158132,6966040,DB703 Anthrazit,1.3,http://www.trilux.com/TOC/6966040,Schutzklasse I,IP65,ET,LED,23,70,1600,3000,TRILUX_Alu_DB703,TRILUX_3000_Skeo_R,TRILUX_Alu_DB703,0.05,Skeo_R_W_LS : TX054490
Skeo R W1 GT SE1R/900-730 1G1P ET,0.1,0.2,0.1,10158130,6965840,DB703 Anthrazit,1.3,http://www.trilux.com/TOC/6965840,Schutzklasse I,IP65,ET,LED,11,70,900,3000,TRILUX_Alu_DB703,TRILUX_3000_Skeo_R,TRILUX_Alu_DB703,0.05,Skeo_R_W_LS : TX054491
Skeo R W1 GT SE1R-SE1R/1800-730 1G1P ET,0.1,0.2,0.1,10158131,6965940,DB703 Anthrazit,1.3,http://www.trilux.com/TOC/6965940,Schutzklasse I,IP65,ET,LED,23,70,1799,3000,TRILUX_Alu_DB703,TRILUX_3000_Skeo_R,TRILUX_3000_Skeo_R,0.0,Skeo_R_W_LS : TX054492
Skeo R W2 GS SE2R/1800-730 1G1P ET,0.15,0.3,0.15,10158140,6966840,DB703 Anthrazit,3.7,http://www.trilux.com/TOC/6966840,Schutzklasse I,IP65,ET,LED,19,70,1799,3000,TRILUX_Alu_DB703,TRILUX_3000_Skeo_R,TRILUX_Alu_DB703,0.075,Skeo_R_W_LS : TX054493
Skeo R W2 GS SE2R-SE2R/3500-730 1G1P ET,0.15,0.3,0.15,10158141,6966940,DB703 Anthrazit,3.7,http://www.trilux.com/TOC/6966940,Schutzklasse I,IP65,ET,LED,38,70,3499,3000,TRILUX_Alu_DB703,TRILUX_3000_Skeo_R,TRILUX_3000_Skeo_R,0.0,Skeo_R_W_LS : TX054494
Skeo R W2 GT SE4R/2000-730 1G1P ET,0.15,0.3,0.15,10158137,6966540,DB703 Anthrazit,3.7,http://www.trilux.com/TOC/6966540,Schutzklasse I,IP65,ET,LED,19,70,1999,3000,TRILUX_Alu_DB703,TRILUX_3000_Skeo_R,TRILUX_Alu_DB703,0.075,Skeo_R_W_LS : TX054495
Skeo R W2 GT SE4R-SE4R/4000-730 1G1P ET,0.15,0.3,0.15,10158138,6966640,DB703 Anthrazit,3.7,http://www.trilux.com/TOC/6966640,Schutzklasse I,IP65,ET,LED,38,70,3999,3000,TRILUX_Alu_DB703,TRILUX_3000_Skeo_R,TRILUX_3000_Skeo_R,0.0,Skeo_R_W_LS : TX054496
