,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,SupEqui##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
SFlow C1-L CDP-I 3700-840 ET 01,1.1315,0.1,0.07,10198402,7354540,RAL9016 Verkehrsweiß,3.6,http://www.trilux.com/TOC/7354540,I,IP20,ET,LED,29,80,66 88 96 90 100 21 47 74 10,3700,4000,C-L_CDP,TRILUX_RAL9016,TRILUX_WH_4000,SFlow_C_LS : TX133379
