,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Opendo D1-L DWW 42-830 ET 03,1.127,0.161,0.045,10241864,7759840,RAL9006 Weißaluminium ,4,http://www.trilux.com/TOC/7759840,I,IP20,ET,LED,28,80,50 83 97 100 100,4000,3000,TRILUX_RAL9006,TRILUX_WH_3000,Opendo_LS : TX277436
