,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Creavo H2-L LW16-03 71-840 ETDD 01,1.209,0.17,0.046,10239839,7736551,RAL9016 Verkehrsweiß,5.8,http://www.trilux.com/TOC/7736551,I,IP20,ETDD,LED,51,80,95 100 100 35 100 32 64 88 65,7100,4000,TRILUX_RAL9016,TRILUX_WH_4000,Creavo_H2_LS : TX278510
