,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Opendo D1-L PW19 36-840 ETDD +LLWM 01,1.127,0.161,0.045,10240274,7744751,RAL9016 Verkehrsweiß ,4.2,http://www.trilux.com/TOC/7744751,I,IP20,ETDD,LED,30,80,65 90 98 99 100 14 43 71 1,3600,4000,TRILUX_RAL9016,TRILUX_WH_4000,Opendo_LS : TX277461
