,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,RegPrim##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Lunexo H2 CDP-I 8800 840 ETDD +LLWS 01,1.503, 0.2, 0.045,10159717,6979651,RAL9016 Verkehrsweiß, 10.5,http://www.trilux.com/TOC/6979651,I,IP20,ETDD,LED,87,80,59 88 97 55 100 50 81 96 45,9000,4000,Lunexo_H_GH,TRILUX_RAL9016,TRILUX_WH_4000,Lunexo_LS : TX054535
