,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,Light Source##OTHER##
InperlaLP C05 BR22 1000-830 ET 01 + DA 01,0.15,0,0.103,10117475,6354940,InperlaLP_DA : 01,RAL9016 Verkehrsweiß,1.317,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6354940,Schutzklasse II,IP20,ET,LED,10,80,82 98 100 100 100,950,3000,TRILUX_Alu_RAL_9016,TRILUX_WH_3000_InperlaLP,TRILUX_BR_InperlaLP,InperlaLP_LS : TX041526
