,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Creavo M84-TS LW19-03 42-830 ET 01,0.622,0.622,0.043,10226125,7639840,RAL9016 Verkehrsweiß ,4.8,http://www.trilux.com/TOC/7639840,II,IP20,ET,LED,25,80,89 100 100 100 100,4000,3000,TRILUX_RAL9016,TRILUX_WH_3000,Creavo_LS : TX195416
