,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##,uff##OTHER##
Bicult Act T SMS TGCS 5500 ETDI QI 01 EU (ActISU),0.32,0.24,0.036,10215601,7520459,RAL9016 Verkehrsweiß,4.16,http://www.trilux.com/TOC/7520459,II,IP20,ETD,LED,46,80,0 0 0 0 100 82 96 100 100,5000,4350,TRILUX_RAL9016,TRILUX_WH_4350,BICULT_LS : TX122134,100
