,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,RegPrim##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
LunexoAct D1 CDP-I 4400 ETDD8 +LLWM 01 ACTDCW,1.203, 0.2, 0.049,10248277,7792962,RAL9016 Verkehrsweiß, 8.9,http://www.trilux.com/TOC/7792962,I,IP20,ETDD8,LED,50,80,60 88 98 99 100 0 0 50 1,4400,6500,Lunexo_D_GH,TRILUX_RAL9016,TRILUX_WH_6500,Lunexo_LS : TX277613
