,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##,uff##OTHER##
Bicult Act T SMC TGCS 5500 ETDI QI 03 EU (ActIWW),0.32,0.24,0.036,10215603,7520659,RAL9006 Weißaluminium,4.16,http://www.trilux.com/TOC/7520659,II,IP20,ETD,LED,48,80,0 0 0 0 100 82 96 100 100,5000,2700,TRILUX_RAL9006,TRILUX_WH_2700,BICULT_LS : TX122156,100
