,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SupEqui_Mat##OTHER##,SupEqui##OTHER##,Light Source##OTHER##
Solegra D3 OTA 13500-830 ET + D3 ZP 05,0.9,0,0.12,10173841 + 10176495,7137840 + 7172000,RAL9016 Verkehrsweiss + RAL9005 Tiefschwarz,12.75,http://www.trilux.com/TOC/7137840,I,IP40 + IP20,ET,LED,89,80,46 78 95 95 100 45 77 94 5,11100,3000,TRILUX_RAL9016,TRILUX_WH_3000_opak,TRILUX_RAL9005,Solegra_D3_ZP : 05,Solegra_LS : TX062786
