,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
CreavoAct M84 LW19-03 42-8 ETDD8 01 (ActDWW),0.622,0.622,0.043,10229000,7617162,RAL9016 Verkehrsweiß ,7.6,http://www.trilux.com/TOC/7617162,I,IP20,ETDD8,LED,35,80,89 100 100 100 100,4200,2700,TRILUX_RAL9016,TRILUX_WH_2700,Creavo_LS : TX195485
