,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,SupEqui##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
SFlow H3-L MRX LED6400-840 ETDD LLWS 01,1.473,0.084,0.045,10148060,6917551,RAL9016 Verkehrsweiß,4.4,http://www.trilux.com/TOC/6917551,I,IP20,ETDD,LED,46,80,84 99 100 69 100 47 80 97 31,6300,4000,H-L_MR_LLW,TRILUX_RAL9016,TRILUX_WH_4000,SFlow_H_LS : TX053184
