,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,SupEqui##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
SFlow H2-L CDP-I 6300-840 ETDD 01,1.413,0.1,0.07,10198450,7358251,RAL9016 Verkehrsweiß,4.65,http://www.trilux.com/TOC/7358251,I,IP20,ETDD,LED,50,80,80 96 99 99 100 27 64 91 1,6300,4000,H-L_CDP,TRILUX_RAL9016,TRILUX_WH_4000,SFlow_H_LS : TX133393
