,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,Light Source##OTHER##
SNS RD7 MRXFL-22 26-840 ETDD 01,0.206,0,0.175,10183641,,RAL9016 Verkehrsweiß,2.9,,I,IP20,ETDD,LED,23,80,79 99 100 100 100,2600,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_MR,Sonnos_LS : TX068828
SNS RD7 MRXFL-22 26-840 ETDD 05,0.206,0,0.175,10183640,,RAL9005 Tiefschwarz,2.9,,I,IP20,ETDD,LED,23,80,79 99 100 100 100,2600,4000,TRILUX_RAL9005,TRILUX_WH_4000,TRILUX_MR,Sonnos_LS : TX068829
SNS RH7-2R MRXFL-22 26-840 ETDD 01,0.206,0,0.175,10183644,,RAL9016 Verkehrsweiß,3.66,,I,IP20,ETDD,LED,23,80,79 99 100 100 100,2600,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_MR,Sonnos_LS : TX068832
SNS RH7-2R MRXFL-22 26-840 ETDD 05,0.206,0,0.175,10183643,,RAL9005 Tiefschwarz,3.66,,I,IP20,ETDD,LED,23,80,79 99 100 100 100,2600,4000,TRILUX_RAL9005,TRILUX_WH_4000,TRILUX_MR,Sonnos_LS : TX068833
