,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO_1##OTHER##,SEO_2##OTHER##,Light Source##OTHER##
Skeo Q-W2 GS RB18R-RB18R/950-840 ETDD (indirect),0.15,0.15,0.15,10192114,7318351,DB703 Anthrazit,2.8,http://www.trilux.com/TOC/7318351,I,IP65,ETDD,LED,16,80,0 0 0 0 100 56 88 99 100,950,4000,TRILUX_RAL703,TRILUX_WH_4000,TRILUX_WH_4000_transp,Skeo_Q_LS : TX084367
