,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,SupEqui##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
SFlow H2-L CDP-I 5300-840 ETDD EB3 03,1.413,0.1,0.07,10198459,7358751,RAL9016 Verkehrsweiß,5.25,http://www.trilux.com/TOC/7358751,I,IP20,ETDD,LED,56,80,66 88 96 62 100 40 71 91 38,6300,4000,H-L_CDP,TRILUX_RAL9016,TRILUX_WH_4000,SFlow_H_LS : TX133416
