,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Regulator##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Nextrema G3 PAW 40-840 ET TWP PC, 1.05, 0.095, 0.105,10228166,7580840,DB703 Anthrazit, 3.1,http://www.trilux.com/TOC/7580840,I,IP66,ET,LED,27,80,44 76 93 96 100 5 13 33 4,4300,4000,Nextrema_G3_Diffusor : XB_B,TRILUX_DB703,TRILUX_WH_4000,Nextrema_G3_LS : TX150196
