,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SEO_2##OTHER##,Light Source##OTHER##
SFlow H2-L MRW LED6400-840 ET 03,1.413,0.084,0.045,10141100,6898740,MRW_MRX : MRW,Weißaluminium RAL 9006,4.09,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6898740,Schutzklasse I,IP20,ET,LED,50,80,6299,4000,TRILUX_Alu_RAL_9006,TRILUX_SFlow_4000,TRILUX_SFlow_4000_outer,Solvan Flow_H_LS : TX050993
