,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Ref##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
7651IP PW 100-830ETDD L150 01,1.474,0.063,0.091,10246612+10241408,9002115592+7789600,RAL9016 Verkehrsweiß,0,http://www.trilux.com/TOC/9002115592,I,IP50+IP50,ETDD,LED,68,80,56 85 95 93 100 15 39 67 7,10000,3000,7651_IP50_P,TRILUX_RAL9016,TRILUX_WH_3000,7651_LS : TX264236
