,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,SupEqui##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
SFlow D2-L CDP-I 4300-830 ET 03,1.413,0.1,0.07,10198431,7356340,RAL9006 Weißaluminium,4.4,http://www.trilux.com/TOC/7356340,I,IP20,ET,LED,37,80,66 88 96 90 100 21 47 74 10,4300,3000,D-L_CDP,TRILUX_RAL9006,TRILUX_WH_3000,SFlow_D_LS : TX133386
