,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,Light Source##OTHER##
SNS QD5 MRVFL-19 20-940 ETDD 05,0.149,0.149,0.175,10183645,,RAL9005 Tiefschwarz,2.1,,I,IP20,ETDD,LED,21,90,96 100 100 100 100,2000,4000,TRILUX_RAL9005,TRILUX_WH_4000,TRILUX_MR,Sonnos_LS : TX068778
SNS QD5 SRVFL-19 20-940 ETDD 01,0.149,0.149,0.175,10183646,,RAL9016 Verkehrsweiß,2.1,,I,IP20,ETDD,LED,21,90,96 100 100 100 100,2000,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_RAL9005,Sonnos_LS : TX068779
SNS QH5-2Q MRVFL-19 20-940 ETDD 05,0.149,0.149,0.175,10183650,,RAL9005 Tiefschwarz,2.66,,I,IP20,ETDD,LED,21,90,96 100 100 100 100,2000,4000,TRILUX_RAL9005,TRILUX_WH_4000,TRILUX_MR,Sonnos_LS : TX068782
SNS QH5-2Q SRVFL-19 20-940 ETDD 01,0.149,0.149,0.175,10183718,,RAL9016 Verkehrsweiß,2.66,,I,IP20,ETDD,LED,21,90,96 100 100 100 100,2000,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_RAL9005,Sonnos_LS : TX068783
