,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,WW##OTHER##,Light Source##OTHER##
InperlaL G2 C07 BR19 2700-840 ETDD 01 + ZN-PC,0.235,0,0.117,10143927;10143989;,6868651;6871700;,InperlaL_C07_ZN-PC,RAL9016 Verkehrsweiß;,1.125,http://www.trilux.com/TOC/6868651,Schutzklasse I,IP40,ETDD,LED,25,80,86 95 98 99 100 22 44 44 1,2699,4000,TRILUX_Alu_RAL_9016,TRILUX_WH_4000_InperlaL,TRILUX_BR_InperlaL,0,InperlaL_C07_LS : TX052850
