,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,Light Source##OTHER##
InperlaLP C05 HR22 1800-840 ETDD EB3 01 + DA-M 03,0.15,0,0.105,10117556,6358951,InperlaLP_DA : M 03,RAL9016 Verkehrsweiß,2.762,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6358951,Schutzklasse I,IP20,ETDD,LED,18,80,79 95 98 100 100 0 0 0 0,1499,4000,TRILUX_Alu_RAL_9016,TRILUX_WH_4000_InperlaLP,TRILUX_HR_InperlaLP,InperlaLP_LS : TX041757
