,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Ref##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
7651IP HE DL 120-865ETDD L150 01,1.474,0.063,0.083,10243748+10241408,9002112588+7789600,RAL9016 Verkehrsweiß,0,http://www.trilux.com/TOC/9002112588,I,IP50+IP50,ETDD,LED,81,80,44 74 92 88 100 12 35 64 12,12600,6500,7651_IP50_DL,TRILUX_RAL9016,TRILUX_WH_6500,7651_LS : TX264191
