,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SupEqui##OTHER##,Light Source##OTHER##
Solegra WD1 OTA 2600-830 ETDD + ZS DB 5075/1500,0.4,0,0.12,10173763 + 10173926,7132951 + 7131400,RAL9016 Verkehrsweiss + RAL9016 Verkehrsweiss,4.85,http://www.trilux.com/TOC/7132951,I,IP40 + IP20,ETDD,LED,19,80,40 70 90 81 100 19 45 72 19,2500,3000,TRILUX_RAL9016,TRILUX_WH_3000_opak,Solegra_WD1_ZS_DB : 5075/1500,Solegra_LS : TX062862
