,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
OleveonF 1.5 L 6000-840 ETDD,1.552,0.102,0.091,10173643,7126551,RAL7035 Lichtgrau,2.6,http://www.trilux.com/TOC/7126551,I,IP66,ETDD,LED,53,80,50 81 94 94 100 0 2 39 6,6300,4000,TRILUX_RAL7035 ,TRILUX_WH_4000,OleveonF_LS : TX056137
